|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| GND | 5V  OUT | GND | 5V  OUT | GND | 5V  OUT |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| VSPD  OUT | I2C  SCL | START  STOP | DIR  IN | RAMP  IN | SPD  IN | GND | 5V  IN |

|  |  |  |
| --- | --- | --- |
| PG  IN | DIR  OUT | I2C  SDA |

|  |  |  |  |
| --- | --- | --- | --- |
| I2C  SCL | I2C  SDA | GND | 5V  IN |